DICOM PS3.3 2020e - Information Object Definitions

A.32.10.2 Real-Time Video Photographic Image IOD Entity-Relationship Model (Current)
Prev | A.32.10 Real-Time Video Photographic Image IOD | Next

#### A.32.10.2 Real-Time Video Photographic Image IOD Entity-Relationship Model

This IOD uses the E-R Model in Section A.1.2, with only the Image IE below the Series IE.

### Note

The Frame Pointers Module is included to managed the temporal synchronization with the video signal the IOD is referring, and optionally the spatial reference if each frame information contains a spatial position.

Prev | Up | Next
A.32.10 Real-Time Video Photographic Image IOD | Home | A.32.10.3 Real-Time Video Photographic Image IOD Module Table

DICOM PS3.3 2020e - Information Object Definitions