DICOM PS3.18 2020e - Web Services

12.6.3.2 Response Header Fields (Current)
Prev | 12.6.3 Response | Next

#### 12.6.3.2 Response Header Fields

Table 12.6.3-2. Response Header Fields

Header Field | Value | Origin Server Usage | Requirement
--- | --- | --- | ---
Content-Type | dicom-media-type | M | The media type of the response payload.
Content-Length | Uint | C | Shall be present if a content encoding has not been applied to the payload.
Content-Encoding | Encoding | C | Shall be present if a content coding has been applied to the payload.

See also Section 8.4.

Prev | Up | Next
12.6.3 Response | Home | 12.6.3.3 Response Payload

DICOM PS3.18 2020e - Web Services