DICOM PS3.3 2020e - Information Object Definitions

C.8.8.6.2 Contour Slab Thickness (Current)
Prev | C.8.8.6 ROI Contour Module | Next

##### C.8.8.6.2 Contour Slab Thickness

A set of Contour slabs may define a multi-slab Volume of Interest. Contour Slab Thickness (3006,0044) shall specify the thickness of a slab, the central plane of which shall be defined by the set of points offset from Contour Data (3006,0050) by the value of Contour Offset Vector (3006,0045). One contour slab may contain one to many sets of Contour Data (3006,0050) that may define regions of one complex Volume of Interest. If no valid value of Contour Slab Thickness (3006,0044) is present, then the offset value shall be (0,0,0) and the original Contour Data (3006,0050) shall define the central plane of the Contour slab.

Prev | Up | Next
C.8.8.6 ROI Contour Module | Home | C.8.8.6.3 Representing Inner and Outer Contours on an Image

DICOM PS3.3 2020e - Information Object Definitions