DICOM PS3.3 2020e - Information Object Definitions

A.34.14.4.7 Waveform Annotation Module (Current)
Prev | A.34.14.4 Electrooculogram IOD Constraints | Next

##### A.34.14.4.7 Waveform Annotation Module

For Concept Name Code Sequence (0040,A043) in Waveform Annotation Sequence (0040,B020) DCID 3037 “EOG Annotations – Neurophysiological Enumerations (EOG)” and DCID 3039 “Device-related and Environment-related Events” shall be used.

### Note

Annotations can be stored either in the Waveform Annotation Module of the waveform to which they apply, or in a separate Structured Report object. The Waveform Annotation Module is only intended for annotations made at the time of acquisition.

Prev | Up | Next
A.34.14.4.6 Waveform Sample Interpretation | Home | A.34.15 Sleep Electroencephalogram IOD

DICOM PS3.3 2020e - Information Object Definitions