DICOM PS3.3 2020e - Information Object Definitions

C.8.22.5.3 PET Detector Motion Details Macro (Current)
Prev | C.8.22.5 Enhanced PET Image Functional Group Macros | Next

##### C.8.22.5.3 PET Detector Motion Details Macro

Table C.8.22-12 specifies the Attributes of the PET Detector Motion Details Functional Group Macro.

Table C.8.22-12. PET Detector Motion Details Macro Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
PET Detector Motion Details Sequence | (0018,9733) | 1 | Contains the Attributes defining the details of the motion of the Detector. Only a single Item shall be included in this Sequence.
>Rotation Direction | (0018,1140) | 1 | Direction of rotation of the detector about the gantry, as viewed while facing the gantry where the table enters the gantry. Enumerated Values: CW clockwise CC counter clockwise
>Revolution Time | (0018,9305) | 1 | The time in seconds of a complete revolution of the detector around the gantry orbit.

Prev | Up | Next
C.8.22.5.2 PET Frame Acquisition Macro | Home | C.8.22.5.4 PET Position Macro

DICOM PS3.3 2020e - Information Object Definitions