DICOM PS3.4 2021b - Service Class Specifications

F.7.2.2 Set Modality Performed Procedure Step Information (Current)
Prev | F.7.2 Operations | Next

#### F.7.2.2 Set Modality Performed Procedure Step Information

This operation allows an SCU to set Attribute Values of an instance of the Modality Performed Procedure Step SOP Class and provide information about a specific real-world Modality Performed Procedure Step that is under control of the SCU. This operation shall be invoked through the DIMSE N-SET Service.

##### F.7.2.2.1 Modality Performed Procedure Step IOD Subset Specification

The Application Entity that claims conformance to this SOP Class as an SCU may choose to modify a subset of the Attributes maintained by the SCP. The Application Entity that claims conformance as an SCP to this SOP Class shall support the subset of the Modality Performed Procedure Step Attributes specified in Table F.7.2-1.

The character set used for Attribute Values updated using the N-SET shall be the same as that specified by the N-CREATE Request Primitive.

Prev | Up | Next
F.7.2 Operations | Home | F.7.2.2.2 Service Class User

DICOM PS3.4 2021b - Service Class Specifications