DICOM PS3.2 2021b - Conformance

I.4.2.3.4 WADO-RS Retrieve Frames (Current)
Prev | I.4.2.3 WADO-RS Specifications | Next

##### I.4.2.3.4 WADO-RS Retrieve Frames

Table I.4.2.3-4. WADO-RS Retrieve Frames

Options | Restrictions
--- | ---
Data Types Supported (Accept Type) | Restricted to application/octet-stream
Transfer Syntaxes Supported (Transfer-syntax Accept parameter) | Any Transfer Syntax supported by the hosting EXAMPLE-PACS-ARCHIVE
SOP Class Restrictions | Restricted to Multi-Frame Image Objects as defined in PS3.3.
Size Restriction | Restricted to size supported by the hosting EXAMPLE-PACS-ARCHIVE

Prev | Up | Next
I.4.2.3.3 WADO-RS Retrieve Instance | Home | I.4.2.3.5 WADO-RS Retrieve Bulk Data

DICOM PS3.2 2021b - Conformance