DICOM PS3.7 2021c - Message Exchange

7.5.3.3 Cancellation (Current)
Prev | 7.5.3 DIMSE Procedures | Next

#### 7.5.3.3 Cancellation

Certain DIMSE services permit the cancellation of the service through the use of service primitives. This allows an invoking DIMSE Service User to request termination of a DIMSE service after completion of the request service primitive but prior to completion of the confirm service primitive.

Table 7.5-2 lists each DIMSE service and its related procedure information. The complete specifications for the service procedures are defined in Sections 9 and 10 for DIMSE-C and DIMSE-N respectively.

Table 7.5-2. DIMSE Services and Procedures

Name | Sub-Operations | Multiple Responses | Cancel
C-STORE | - | - | -
C-GET | M | C | M
C-MOVE | M | C | M
C-FIND | - | C | M
C-ECHO | - | - | -
N-EVENT-REPORT | - | - | -
N-GET | - | - | -
N-SET | - | - | -
N-ACTION | - | - | -
N-CREATE | - | - | -
N-DELETE | - | - | -

Prev | Up | Next
7.5.3.2 Multiple Responses | Home | 8 Protocol Overview

DICOM PS3.7 2021c - Message Exchange