DICOM PS3.7 2021c - Message Exchange

5 Conventions (Current)
Prev |  | Next

# 5 Conventions

The following conventions are used for the service description tables shown in this Part of the Standard.

(=)

  The value of the parameter is equal to the value of the parameter in the column to the left.

-

  Not applicable. The parameter shall not be present.

C

  The parameter is conditional. The condition(s) are defined by the text that describes the parameter.

M

  Mandatory usage

MF

  Mandatory with a fixed value

U

  The use of this parameter is a DIMSE Service User option

UF

  User Option with a fixed value

Prev |  | Next
4 Symbols and Abbreviations | Home | 6 Service Context

DICOM PS3.7 2021c - Message Exchange