DICOM PS3.4 2021c - Service Class Specifications

GG.6.4 CT and XA Defined Procedure Protocol Storage SOP Class (Current)
Prev | GG.6 Application Behavior for Standard SOP Classes | Next

### GG.6.4 CT and XA Defined Procedure Protocol Storage SOP Class

An implementation that conforms to the CT and/or XA Defined Procedure Protocol Storage SOP Classes as an SCP shall not modify constraints for which the value of the Modifiable Constraint Flag (0082,0038) is NO.

Modifying protocol constraints changes the semantics of a CT or XA Defined Procedure Protocol Storage SOP Instance.

Prev | Up | Next
GG.6.3 Template Storage SOP Classes | Home | GG.6.5 Protocol Approval Storage SOP Class

DICOM PS3.4 2021c - Service Class Specifications