DICOM PS3.18 2021d - Web Services

I Store Instances Response Module (Current)
Prev |  | Next

# I Store Instances Response Module

## I.1 Response Message Body

Table I.1-1 defines the Attributes for referencing SOP Instances that are contained in a Store Instances Response Module in the response message body.

Table I.1-1. Store Instances Response Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Retrieve URL | (0008,1190) | 2 | The URL where the Study is available for retrieval via a Studies Retrieve Transaction (Section 10.4). ### Note The VR of this attribute has changed from UT to UR.
Failed SOP Sequence | (0008,1198) | 1C | A Sequence of Items where each Item references a single SOP Instance for which storage could not be provided. Required if one or more SOP Instances failed to store.
>Table 10-11 “SOP Instance Reference Macro Attributes” in PS3.3
>Failure Reason | (0008,1197) | 1 | The reason that storage could not be provided for this SOP Instance. See Section I.2.2.
Referenced SOP Sequence | (0008,1199) | 1C | A Sequence of Items where each Item references a single SOP Instance that was successfully stored. Required if one or more SOP Instances were successfully stored.
>Table 10-11 “SOP Instance Reference Macro Attributes” in PS3.3
>Retrieve URL | (0008,1190) | 2 | The URL where the SOP Instance is available for retrieval via a Studies Retrieve Transaction (Section 10.4). ### Note The VR of this attribute has changed from UT to UR.
>Warning Reason | (0008,1196) | 1C | The reason that this SOP Instance was accepted with warnings. Required if there was a warning for this SOP Instance. See Section I.2.1.
>Original Attributes Sequence | (0400,0561) | 3 | Sequence of Items containing all attributes that were removed or replaced by other values. One or more Items are permitted in this sequence.
>>Attribute Modification DateTime | (0400,0562) | 1 | Date and time the attributes were removed and/or replaced.
>>Modifying System | (0400,0563) | 1 | Identification of the system that removed and/or replaced the attributes.
>>Reason for the Attribute Modification | (0400,0565) | 1 | Reason for the attribute modification. Defined Terms COERCE Replace values of attributes such as Patient Name, ID, Accession Number, for example, during import of media from an external institution, or reconciliation against a master patient index. CORRECT Replace incorrect values, such as Patient Name or ID, for example, when incorrect worklist item was chosen or operator input error.
>>Modified Attributes Sequence | (0400,0550) | 1 | Sequence that contains all the Attributes, with their previous values, that were modified or removed from the main Data Set. Only a single Item shall be included in this sequence.
>>Any Attribute from the main Data Set that was modified or removed; may include Sequence Attributes and their Items.
Other Failures Sequence | (0008,119A) | 1C | Reasons not associated with a specific SOP Instance that storage could not be provided. Each Item references a single storage failure. Required if there are one or more failures not associated with a specific SOP Instance.
>Failure Reason | (0008,1197) | 1 | The reason that storage could not be provided for this message item. See Section I.2.2.

Prev |  | Next
H Capabilities Description | Home | I.2 Store Instances Response Attribute Description

DICOM PS3.18 2021d - Web Services