DICOM PS3.16 2021d - Content Mapping Resource

TID 10049 Radiation Field Area (Current)
Prev | Enhanced X-Ray Radiation Dose SR IOD Templates | Next

### TID 10049 Radiation Field Area

This template contains a description of the radiation field area for a given X-Ray source, which accounts for collimation.

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 10049. Radiation Field Area

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (130516, DCM, "Radiation Field Area") | 1 | M |  |
2 | > | CONTAINS | DATETIME | DT (111526, DCM, "DateTime Started") | 1 | M |  |
3 | > | CONTAINS | DATETIME | DT (111527, DCM, "DateTime Ended") | 1 | M |  |
4 | > | CONTAINS | TEXT | EV (113832, DCM, "Identification of the X-Ray Source") | 1 | M |  |
5 | > | CONTAINS | SCOORD3D | EV (130517, DCM, "Radiation Field Outline") | 1-n | M |  | GRAPHIC TYPE = {POLYGON, ELLIPSE}
6 | >> | HAS PROPERTIES | CODE | EV (130518, DCM, "Value Timing") | 1 | U |  | DCID 10073 “Value Timings”

Content Item Descriptions

Row 2 | The DateTime of the beginning of the time period over which the content items are applicable.
Row 3 | The DateTime of the end of the time period over which the content items are applicable.
Row 4 | Identification the X-Ray source. This designation shall not change for a given source throughout the entire RDSR.
Row 5 | The Radiation Field Outline describes the area and shape of the radiation field. The points shall be coplanar and are defined in the X-Ray source reference coordinate system.

Prev | Up | Next
TID 10048 Radiation Output | Home | TID 10050 X-Ray Source Reference Coordinate System

DICOM PS3.16 2021d - Content Mapping Resource