DICOM PS3.4 2021d - Service Class Specifications

Z.3 Standard Composite Instance Retrieve Without Bulk Data Information Model (Current)
Prev | Z Composite Instance Retrieve Without Bulk Data Service Class (Normative) | Next

## Z.3 Standard Composite Instance Retrieve Without Bulk Data Information Model

One standard Composite Instance Retrieve Without Bulk Data Information Model is defined in this Annex. The Composite Instance Retrieve Without Bulk Data Information Model is associated with a single SOP Class. The following Composite Instance Retrieve Without Bulk Data Information Model is defined:

- Retrieve Without Bulk Data

### Z.3.1 Composite Instance Retrieve Without Bulk Data Information Model

The Composite Instance Retrieve Without Bulk Data Information Model is based upon a one level hierarchy:

- Composite Instance

The Retrieve Without Bulk Data Information Model may be represented by the entity relationship diagram shown in Figure Z.3.1-1.

Figure Z.3.1-1. Retrieve Without Bulk Data Information Model E/R Diagram

The Composite Instance level is the only level and contains only the SOP Instance UID.

Prev | Up | Next
Z.2.2 Attributes Definition | Home | Z.4 DIMSE-C Service Groups

DICOM PS3.4 2021d - Service Class Specifications