DICOM PS3.4 2021d - Service Class Specifications

S.3 Media Creation Management SOP Class (Current)
Prev | S Media Creation Management Service Class (Normative) | Next

## S.3 Media Creation Management SOP Class

The SCU transmits the SOP Instances to the SCP using the Storage Service Class. The request for media creation is transmitted to the SCP and contains a list of references to one or more SOP Instances. Success or failure of media creation is subsequently indicated by the SCU requesting the status from the SCP on the same or a separate association.

### S.3.1 DIMSE Service Group

The following DIMSE-N Services are applicable to the Media Creation Management SOP Class.

Table S.3.1-1. DIMSE Service Group Applicable to Media Creation Management

DICOM Message Service Element | Usage SCU/SCP
--- | ---
N-CREATE | M/M
N-ACTION | M/M
N-GET | U/M

The DIMSE-N Services and Protocol are specified in PS3.7.

Prev | Up | Next
S.2 Conformance Overview | Home | S.3.2 Operations

DICOM PS3.4 2021d - Service Class Specifications